REFERENCE DATA:

1:Suitable applications: Water. Oil. Gas.

2:Design&Manufacture: API 609 , ASME/ANSI B16.34,JIS B2220,JIS B2031,BS 5155

3:F TO F dimensions: JIS B2002,ASME B16.10

4:Connection: Drilled according to JIS B2220-5/10/20K, ASME/ANSI B16.5 & B16.47 A/B series,BS 4504 double flanges are available .

5:Seat structure: Vulcanized rubber..

6:Pressure rating : PN16/150LB/JIS16K and below.

7:Size: 2" and above.

8:Sealing structure: Rubber seal

9:Safety design: anti-static

10:Inspection and approval norm: API598,API6D .

QUALITY CONTROL:

1. 100% Chemical analysis and mechanical test with raw materials of each heat numbers.

2.100% DPT test with the castings, partly MT or UT test , RT is always available if required.

3.100% hydraulic test with the shell and seal and low pressure air test.

GUATANTEE:

IMD provide 12 months service life at least , free spares and maintance instruction will be provided when required.