REFERENCE DATA:

1:Suitable applications: Water. Oil. Gas.

2:Design&Manufacture: API 6D , API600, ASME/ANSI B16.34

3:F TO F dimensions: ASME/ANSI B16.10 and factory standard

4:Connection: ASME/ANSI B16.5 & B16.47 A/B series. BW,RTJ are available .

5:Bonnet structure: Bolted or Pressure Seal

6:Pressure rating :150LB and above

7:Size: 26" and above.

8:Sealing structure: metal seal covered with stellite hard face to get reliable performance and service life.

9:Safety design: Manual override,IP65 and above,Ex-proof etc.

10:Inspection and approval norm: API598,API6D .

11:Power of actuator: 110/220/230/380/400/440/480VAC,3PH.56/60HZ etc.

12:Output torques of actuator: 27000N.M MAX.

QUALITY CONTROL:

1. 100% Chemical analysis and mechanical test with raw materials of each heat numbers.

2.100% DPT test with the castings, partly MT or UT test , RT is always available if required.

3.100% hydraulic test with the shell and seal and low pressure air test.

GUATANTEE:

IMD provide 12 months service life at least , free spares and maintance instruction will be provided when required.