CLIMAX PLUG VALVE LUBRICANT & SEALANT

STANDARD TEMPERATURE SERVICES 32’F TO 250’F

DESIGNED SPECIALLY FOR LUBRICATING FMC WECO PLUG VALVES.

Valves must be lubricated on routine basis for best sealing performance and corrosion protection. Valves should be flushed with clean water and regreased after each use. Periodic disassembly of valve is necessary to remove contaminated grease.

Grease valve in open position until grease can be seen to come into through bore of valve. Cycle valve closed and open and pump a little more grease into open position. If valve is in a line grease valve a moderate amount after maximum grease pressure is attained during greasing, then cycle valve and regrease.

NOTE: TYPICAL PRESSURE ATTAINED DURING GREASING OF VALVE RANGE FROM 6000 PSI TO 20,000 PSI.