|  |
| --- |
| FOR WEB |
| **GATE VALVE:**  We can offer a complete range of Gate Valve for drilling and production applications. We have in-house facility for testing of Valve. We can provide customers with reliable inspection, repair and certification services for all types of high pressure gate valves and manifolds. These services can be provided infield, in customer yards or in our workshops as required.  **FEATURES:**   * Slab design suitable for actuation and compatible with a wide range of actuators * Working pressure ratings of 5000 to 15,000 psi. * Positive Metal to Metal sealing (gate-to-seat and seat-to-body) * Bi-directional sealing design * Full bore through conduit construction. * Long life of Gate & Seals * Components constructed of various alloys and coatings for severe service applications. * Forged body & bonnet for the highest mechanical integrity * Can be equipped with pneumatic & hydraulic actuators      |  |  |  |  | | --- | --- | --- | --- | | **SIZE (Inches)** | **PRESSURE** | | | | **5,000 PSI** | **10,000 PSI** | **15,000 PSI** | | 2-1/1’’ |  |  |  | | 3-1/8’’ |  |  |  | | 3-1/16’’ |  |  |  | | 4-1/16’’ |  |  |  | |