|  |
| --- |
| FOR WEB: |
| **PLUG VALVE:**We can offer high pressure low torque Plug Valves available in size from 1 to 4 inches. They come in multiple bores and are available up to 15,000 PSI for standard service and 10,000 PSI for H2S or sour gas service. They come with threaded & wing nut union.Our plug valves are pressure balanced type and have replaceable metal liners between the body and plug. Repair kits are also available to increase their life and make them perform safely for longer. These Plug Valves are designed to meet the needs and requirements of the drilling, production & well-servicing applications. They can withstand the high erosion rates and pressures encountered in today’s operating environment.**FEATURES:*** Two-piece floating plug/stem
* Fast, simple field repair
* Eliminates body washout, extends body life
* Handles sand & cement
* Interchangeable design
* Eliminates corrosion in segment sealing area
 |
| **REPAIR KIT :****We can provide Plug valve repair kits of FMC Technologies, SPM & NOV** for standard service, or low temperature and sour gas condition. These **repair kits** are replaceable and interchangeable for SPM, **FMC** 2” and 3” DR & ULT **plug Valve**, which is including **plug**, seal segment, side segment, elastomer seals, and grease fittings. |