|  |
| --- |
| FOR WEB: |
| **ADAPTER & CROSSOVER :**  We offers adapter crossover and changeovers in integral, threaded and welded construction for sizes upto 5 inch in different combination as per customer requirement. These crossover are manufactured for pressure rating upto 15,000 PSI. |