|  |
| --- |
| FOR WEB |
| **PUP JOINTS :**  We offers Pup Joints with Integral Hammer Union end connections. These Pup joints are used on high pressure discharge lines, choke and kill lines, auxiliary flow and other application. These light weight pup joints are available in lengths ranging 1 feet to 12 feet and sizes from 2 inch to 4 inch for pressure rating 6000 to 15000 PSI.  We also offer pup joints in welded, NPST and NPT (Threaded) construction as per customer requirement. |