|  |
| --- |
| FOR WEB |
| **RING JOINTS GASKETS**We offers a large variety of ring joint gaskets. The RTJ standard size gaskets are offered in accordance to API – 6A and ASME B16.20 specification. These gaskets are manufactured in various types, comprising of R type (Oval & Octagonal), RX type, BX type, in Low carbon steel, soft iron, stainless steel (SS304L,SS316L). |