|  |
| --- |
| FOR WEB: |
| Digant Energy offer the following features.   * Minimum flow restriction * Available for standard and sour service * All sizes are available in 8 styles, for 360 rotation in 1, 2 or 3 planes * Heavy duty hex head style ball loading plug * Grease retainer ring (ensures clean ball race) * Standard packing units (operating temperature to 225 °F) * Superior hardened ball races ensure uniform surface hardness and depth for longer life under severe thrust and radial loading * Other end connections are available on request |