|  |
| --- |
| FOR WEB: |
| Digant Energy offer the following features.* Minimum flow restriction
* Available for standard and sour service
* All sizes are available in 8 styles, for 360 rotation in 1, 2 or 3 planes
* Heavy duty hex head style ball loading plug
* Grease retainer ring (ensures clean ball race)
* Standard packing units (operating temperature to 225 °F)
* Superior hardened ball races ensure uniform surface hardness and depth for longer life under severe thrust and radial loading
* Other end connections are available on request
 |